{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":5,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":10,"n_cols":7,"rows_kept":10,"cut":false,"hidden":false,"merged":[[9,0,9,2],[9,4,9,6],[0,0,1,6]],"flags":["formulas_cached_only"]}
["环能净水空压机维保清单"]
[]
[]
["序号","品牌","规格型号","数量","维保内容","备注","设备铭牌"]
[1,"捷豹","XS-1078",4,"保养周期为设备每运行2000小时进行一次保养，更换空气过滤器、油过滤器、油气分离器、螺杆空压机专用润滑油、电机润滑脂;对连接件进行紧固;调整或更换三角带;进行设备内部清洁;检查是否有异常声音、振动;检查电器元件老化情况及电缆绝缘、接地情况等。","一厂2台、二厂2台"]
[2,"博莱特","MODELTH-37/8",2,"保养周期为设备每运行2500小时进行一次保养，更换空气过滤器、油过滤器、油气分离器、螺杆空压机专用润滑油、电机润滑脂;对连接件进行紧固;调整或更换三角带;进行设备内部清洁;检查是否有异常声音、振动;检查电器元件老化情况及电缆绝缘、接地情况等。","一厂"]
[3,"富达","LUD-57-R",1,"保养周期为设备每运行2500小时进行一次保养，更换空气过滤器、油过滤器、油气分离器、螺杆空压机专用润滑油、电机润滑脂;对连接件进行紧固;调整或更换三角带;进行设备内部清洁;检查是否有异常声音、振动;检查电器元件老化情况及电缆绝缘、接地情况等。","二厂"]
[4,"富达","LY30-10",1,"保养周期为设备每运行2500小时进行一次保养，更换空气过滤器、油过滤器、油气分离器、螺杆空压机专用润滑油、电机润滑脂;对连接件进行紧固;调整或更换三角带;进行设备内部清洁;检查是否有异常声音、振动;检查电器元件老化情况及电缆绝缘、接地情况等。","二厂"]
[5,"博莱特","MODELTH-45PM+",1,"保养周期为设备每运行2500小时进行一次保养，更换空气过滤器、油过滤器、油气分离器、螺杆空压机专用润滑油、电机润滑脂;对连接件进行紧固;调整或更换三角带;进行设备内部清洁;检查是否有异常声音、振动;检查电器元件老化情况及电缆绝缘、接地情况等。","二厂"]
["合计数量",null,null,9,"服务周期为一年（自合同签订之日起算）"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}